# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title: Supply of music instrument – GRAND PIANO p 1 /3**

**Publication reference:** SUP 2019-1

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments on its proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.**  **Item number** | **2.**  **Specifications required** | **3.**  **Specifications offered** | **4.**  **Notes, remarks,  ref to documentation** | **5.**  **Evaluation committee’s notes** |
| --- | --- | --- | --- | --- |
| **1** | Length: 275 cm - 279 cm |  |  |  |
| **2** | Width: 158 cm - 162 cm |  |  |  |
| **3** | Weight: minimum 500 kg |  |  |  |
| **4** | Finish: Polished Ebony or equivalent, Hard Finish resistance on scratch |  |  |  |
| **5** | Bench: Height Adjustable |  |  |  |
| **6** | Sound board material: a wood having stability and vibrance under stress and vibration which is used exclusively for the soundboard: resonance spruce wood or equivalent |  |  |  |
| **7** | Bass strings: hand coiled |  |  |  |
| **8** | Hammers: hand made, Double Felted |  |  |  |
| **9** | Agraffes:  Special handmade brass agraffes or equivalent |  |  |  |
| **10** | Dampers:  with high efficiency dual pivot construction for smoother half pedal control |  |  |  |
| **11** | Beams:  Made from durable spruce - one piece selected beams to support strength of construction |  |  |  |
| **12** | Key Action description:  Millenium III advance with 30% more in dynamics (compare with classical mechanic construction) like, with extended Length of key stick to minimum of 54 cm, F like Hammer Rail, with use of only high efficiency machine screws to set up hammers on rail, with minimum of six (6) Rail Holders for complete hammers setup, Black Jack construction from ABS Styran, extremely resistance to changes in humidity and temperature, **or equivalent function and quality of Key Action** |  |  |  |
| **13** | Warranty: 60 months |  |  |  |